22 April 2003 JAC Pole Geometries and Currents Used for Field Calculations

7-Pole Wiggler (1.9 T Peak Field) – Wiggler #1 – Version 37 135 – Pole Length Number Cutout Width Cutout Depth Main Current Main Turns Main Width Trim Current Trim Turns Trim Width (cm) (cm) (mm) (Amp-turns) (Inches) (Amp-turns) (Inches) 20 5 6 5.0 79.38k 588 1.000 —– —– —– 15 2 6 3.5 51.03k 378 0.642 1.33k 663 0.358

7-Pole Wiggler (2.1 T Peak Field) – Wiggler #1 – Version 37 161 – Pole Length Number Cutout Width Cutout Depth Main Current Main Turns Main Width Trim Current Trim Turns Trim Width (cm) (cm) (mm) (Amp-turns) (Inches) (Amp-turns) (Inches) 20 5 6 5.0 95.00k 588 1.000 —– —– —– 15 2 6 3.5 61.07k 378 0.642 0.86k 663 0.358

7-Pole Wiggler (2.1 T Peak Field) – Wiggler #2 – Version 44 144 – Pole Length Number Cutout Width Cutout Depth Main Current Main Turns Main Width Trim Current Trim Turns Trim Width (cm) (cm) (mm) (Amp-turns) (Inches) (Amp-turns) (Inches) 20 5 6 5.0 95.00k 660 1.000 —– —– —– 15 2 6 3.6 57.00k 396 0.603 4.569k 684 0.380

8-Pole Wiggler (2.1 T Peak Field) – Wiggler #3 – Version 37 144 – Pole Length Number Cutout Width Cutout Depth Main Current Main Turns Main Width Trim Current Trim Turns Trim Width (cm) (cm) (mm) (Amp-turns) (Inches) (Amp-turns) (Inches) 20 4 6 5.0 95.00k 660 1.000 —– —– —– 15 2 6 5.5 95.00k 660 1.000 —– —– —– 10 2 6 3.6 50.67k 352 0.533 0.993k 836 0.467