0 50 100 150 200 0 1 2 3 4 5 6 7 8

Beam current (mA) collector current density (nA/mm 2)

NEG Coated Drift Chamber RFA #3, 1x20 e+, 5.3GeV, 14ns

4/25/10 (before activation) 4/29/10 (after activation) 7/20/10 (after CHESS run)