{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["RFA List","RFA Styles","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"RFA List","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["RFA Long Name","Short Name","Location (m)","RFA Style","Beam Pipe","Mitigation","Field (T)","File Name Base","Notes"]
["D01W_RFA1_SEG_TiN-Cu","Seg1W",0.737,"Insertable Segmented","Cu","TiN",0,"RFA_01W_G3","In wiggler fringe field?"]
["SCW01W_RFA1_WIG1_NM-Cu","Wig1W Con A",1.66,"Wiggler1","Cu","none","?","RFA_01W_G1","In wiggler longitudinal field"]
["SCW01W_RFA2_WIG1_NM-Cu","Wig1W Con B",1.758,"Wiggler1","Cu","none",1.9,"RFA_01W_G1","In wiggler pole center"]
["SCW01W_RFA3_WIG1_NM-Cu","Wig1W Con C",1.91,"Wiggler1","Cu","none","?","RFA_01W_G1","In wiggler intermediate field"]
["SCW02WA_RFA1_WIG1_TiN-Cu","Wig2A Con A",4.381,"Wiggler1","Cu","TiN","?","RFA_01W_G1","In wiggler longitudinal field"]
["SCW02WA_RFA2_WIG1_TiN-Cu","Wig2A Con B",4.481,"Wiggler1","Cu","TiN",1.9,"RFA_01W_G1","In wiggler pole center"]
["SCW02WA_RFA3_WIG1_TiN-Cu","Wig2A Con C",4.631,"Wiggler1","Cu","TiN","?","RFA_01W_G1","In wiggler intermediate field"]
["SCW02WB_RFA1_WIG2_Elct-Cu","Wig2B Con A",6.111,"Wiggler2","Cu","Electrode","?","RFA_01W_G2","In wiggler longitudinal field"]
["SCW02WB_RFA2_WIG2_Elct-Cu","Wig2B Con B",6.21,"Wiggler2","Cu","Electrode",1.9,"RFA_01W_G2","In wiggler pole center"]
["SCW02WB_RFA3_WIG2_Elct-Cu","Wig2B Con C",6.36,"Wiggler2","Cu","Electrode","?","RFA_01W_G2","In wiggler intermediate field"]
["D12W_RFA1_CVC1_NM-Al ","Thin B12WS",67.56,"Thin1","Al","none",0,"RFA_13W_G2","In dipole fringe field?"]
["B12W_RFA2_CVC1_NM-Al ","Dipole B12WN",74.019,"Thin1","Al","none",".0790-.1896","RFA_13W_G2","Field depends on beam energy"]
["D14BW_RFA1_APS_NM-Cu","APS South",87.99,"APS","Cu","none",0,"RFA_13W_G3"]
["D14BW_RFA2_SEG_NM-Cu","Seg 14BWS",88.09,"Insertable Segmented","Cu","none",0,"RFA_13W_G1"]
["D14BW_RFA3_APS_NM-Cu","APS North",88.195,"APS","Cu","none",0,"RFA_13W_G3"]
["D14BW_RFA4_SEG_NM-Cu","Seg 14BWN",89.78,"Insertable Segmented","Cu","none",0,"RFA_13W_G1"]
["D15W_RFA1_CVC2_TiN-Al","Thin 15W",100.328,"Thin2","Al","TiN",0,"RFA_13W_G2"]
["Q48W_RFA1_Quad1_NM-Al","Quadrupole",379.05,"Quadrupole","Al","none",null,"RFA_L3a_G2"]
["CHC48W_RFA1_SLAC1_GrTiN-Al","SLAC1",380.95,"SLAC","Al","Grooves, TiN","0-.12","RFA_L3a_G1","Chicane RFA"]
["CHC48W_RFA2_SLAC1_TiN-Al","SLAC2",381.73,"SLAC","Al","TiN","0-.12","RFA_L3a_G1","Chicane RFA"]
["CHC48W_RFA3_SLAC1_TiN-Al","SLAC3",382.46,"SLAC","Al","TiN","0-.12","RFA_L3a_G1","Chicane RFA"]
["CHC48W_RFA4_SLAC1_NM-Al","SLAC4",383.2,"SLAC","Al","none","0-.12","RFA_L3a_G1","Chicane RFA"]
["D48E_RFA2_APS_NEG_SS","D48E RFA2",390,"APS","SS","NEG",0,"RFA_L3a_G3","located opposite source point"]
["D48E_RFA3_APS_NEG_SS","D48E RFA3",390,"APS","SS","NEG",0,"RFA_L3a_G3","located 135 degrees from source point"]
["D48E_RFA4_APS_NEG_SS","D48E RFA4",390,"APS","SS","NEG",0,"RFA_L3a_G3","located 45 degrees from source point"]
["D15E_RFA1_CVC2_aC-Al","Thin 15E",667.88,"Thin2","Al","Carbon",0,"RFA_14E_G2"]
["D14BE_RFA2_SEG_ TiN-Cu","Seg 14EN",680.49,"Insertable Segmented","Cu","TiN",0,"RFA_14E_G1"]
["D14BE_RFA1_SEG_ NM-Cu ","Seg 14ES",682.17,"Insertable Segmented","Cu","none",0,"RFA_14E_G1"]
["D02E_RFA1_SEG_NM_Cu","Seg 2E",761.19,"Insertable Segmented","Cu","none",0,"RFA_01W_G3"]

{"sheet":"RFA Styles","index":1,"n_rows":25,"n_cols":15,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Style","Alias(es)","# Retarding Grids","# Ground Grids","# Collectors","Beam hole area (mm^2)","Grid Trans. ","Col Area (mm^2)","Scan Grid","Col. Width (mm)","Col Spacing (mm)","Total Width (mm)","Length (mm)","Beam Pipe Trans.","Notes"]
["Insertable Segmented","SEG",1,1,5,228,0.38,6.58464,2,6,6,54,40,0.18]
["Thin1","Dipole, CVC1",3,0,9,205.48,0.38,8.675822222222221,1,3,4.2,60.6,32,0.22,"Grids are arranged transversely"]
["Thin2","CVC2",3,0,9,205.48,0.9,20.548,1,3,4.2,60.6,32,0.22,"Grids are arranged transversely"]
["Wiggler1","WIG1",1,0,12,109.42,0.38,3.4649666666666668,1,1.9,1.5,39.3,28,0.17]
["Wiggler2","WIG2",1,0,12,109.42,0.9,8.2065,1,1.9,1.5,39.3,28,0.17]
["APS",null,1,1,1,87.7,0.46,18.55732,2,19.8,0,19.8,24.3,0.18]
["SLAC","SLAC1",1,2,17,617.2,0.9,26.46698823529412,1,2.9,0,49.3,58,0.23]
["Quadrupole","Quad1",1,1,12,902.8,0.9,60.939,1,2.17,3,59.04,124,0.28,"Collectors are arranged azimuthally, see table below"]
[]
[]
["Quadrupole RFA","Collectors span the azimuthal region between Phi_1 and Phi_2.  Zero degrees is the source point (outer edge)."]
["Collector #","Phi_1 (degrees)","Phi_2 (degrees)"]
[1,71.6,74.39999999999999]
[2,78.3,81.1]
[3,85,87.8]
[4,91.7,94.5]
[5,98.4,101.2]
[6,105.10000000000001,107.9]
[7,113.70000000000002,116.50000000000003]
[8,120.40000000000002,123.20000000000002]
[9,127.10000000000002,129.9]
[10,133.8,136.60000000000002]
[11,140.5,143.3]
[12,147.2,150]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}