{"text_format":"2","workbook":"xls","n_sheets":6,"sheets":["down by region","down by system chart","down by component name","down by system list","down by region list","resultsXFEL22"],"not_rendered":{"charts":2,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"down by region","index":0,"reason":"not_a_worksheet"},{"sheet":"down by system chart","index":1,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"down by component name","index":2,"n_rows":80,"n_cols":2,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
["Sum of % down * 100"]
["comp name  ","Total"]
["Power supplies SC quad beamline",323.9]
["cryo plant beamline",131.4]
["site power beamline",69.9]
["Quads beamline",47.7]
["Vac Mech device beamline",36.5]
["Electrical - .05<<0.5 Utility power",34.7]
["local backbone sector",25.5]
["Central Water beamline",24.9]
["Controls sitewide beamline",23.8]
["Power supplies strings beamline",19.7]
["MPS & FastFdbk region",14.4]
["Flow Switch - quads beamline",13.8]
["Klystrons klystron",13.5]
["VacV controller beamline",12.5]
["PS controller - corr can tune around beamline",11.7]
["insulating vacuumP cryo string",11.6]
["PS controller SC quad beamline",11.4]
["Kicker pulser beamline",9.6]
["VacP power supply coupler",8.8]
["coupler interlock sensors coupler",8.8]
["PS controller string beamline",8]
["PS Corrs can tune around beamline",7.9]
["other controls klystron",7.6]
["Modulators klystron",7.2]
["coupler interlock electronics coupler",6.9]
["VacV beamline",4.5]
["VacP power supply klystron",3.4]
["timing klystron",3]
["Pulse transformers klystron",2.5]
["pulse cables klystron",2.3]
["LLRF klystron",2.3]
["Controls PPS region",2.2]
["power coupler coupler",1.9]
["VacG/Ctrl klystron",1.7]
["schedMaintn",1.4]
["klys pre-amp klystron",1.3]
["cryo JT valve cryo string",1.3]
["timing sector",1.1]
["controls backbone sector",1]
["VacP power supply beamline",0.8]
["laser beamline",0.7]
["VacP coupler",0.5]
["Kickers beamline",0.4]
["Corrs - can tune around beamline",0.4]
["Electrical - >0.5 klystron",0.4]
["Flow Switch klystron",0.3]
["Quads SC beamline",0.3]
["PS controller - corr can't tune around beamline",0.3]
["Laser PS beamline",0.2]
["Electrical - .05<<0.5 klystron",0.2]
["other controls beamline",0.1]
["(blank)"]
["quad or corr beamline",0]
["Quad/Sext trims beamline",0]
["Cavity tuner cavity",0]
["BPMs diagnostic",0]
["Kicker diagnostic",0]
["Cavity piezo tuner cavity",0]
["spare klystron klystron",0]
["timing beamline",0]
["PS Corrs can't tune around beamline",0]
["Electrical - .05<<0.5 beamline",0]
["Undulator movers beamline",0]
["cryo vac enclosure cryo segment",0]
["LLRF cavity",0]
["VacP beamline",0]
["Corrs - can't tune around beamline",0]
["VacP klystron",0]
["power coupler disc coupler",0]
["Electrical - >0.5 beamline",0]
["Power supplies Trims beamline",0]
["Kicker pulser diagnostic",0]
["Cavities cavity",0]
["Wigglers beamline",0]
["wire scanners diagnostic",0]
["Grand Total",926.2]

{"sheet":"down by system list","index":3,"n_rows":18,"n_cols":2,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["This is a pivot table.  You can double click on an item to get more detail"]
[]
["Sum of % down * 100"]
["         system","Total"]
["PS + controllers",392.7]
["          lumped",250]
["        controls",57.2]
["          Vacuum",54.3]
["         Magnets",48.8]
["        AC power",35.3]
["RF power sources",31.9]
["    RF structure",26.9]
["    Water system",14.1]
["            Cryo",12.9]
["      schedMaint",1.4]
["      Diagnostic",0.7]
["(blank)"]
["Grand Total",926.2]

{"sheet":"down by region list","index":4,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["This is a pivot table.  You can double click on an item to get more detail"]
[]
["Sum of % down * 100"]
["       region","Total"]
["   main linac",414.8]
["  Cryo plants",131.4]
[" compressor 2",85.7]
["   Site power",69.9]
[" compressor 1",55.7]
["   injector 1",47.7]
["       SASE 2",42.1]
["       SASE 1",28.8]
["Central Water",24.9]
["Global controls",23.8]
["    all users",1.4]
["(blank)"]
["Grand Total",926.2]

{"sheet":"resultsXFEL22","index":5,"n_rows":408,"n_cols":15,"rows_kept":408,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["14:22 XFEL3 but 8+ 8 hour sched down frac down*1e4","n failures causing down","n failures ignored","n failures not ignored","comp name  ","       region","   subregion","         system","  ","region   "," % downtime incl forced MD"," % allowd opp MD"," % actual opp MD"," %desired MD"," %sched MD"]
[0.7,4,2,4,"laser beamline","   injector 1","       laser","      Diagnostic"]
[0.2,1,0,1,"Laser PS beamline","   injector 1","       laser","PS + controllers","  ","          Site power",0.6988,0.1775,0,0,0]
[1.9,2,1,2,"Vac Mech device beamline","   injector 1","       laser","          Vacuum","  ","       Central Water",0.2488,0.9527,0,0,0]
[0,0,0,0,"VacP beamline","   injector 1","       laser","          Vacuum","  ","         Cryo plants",1.314,0.1681,0,0,0]
[0.8,8,3,8,"VacP power supply beamline","   injector 1","       laser","          Vacuum","  ","     Global controls",0.2383,0.2201,0,0,0]
[0,0,0,0,"VacV beamline","   injector 1","       laser","          Vacuum","  ","          injector 1",0.4744,3.578,1,1,0]
[0.9,4,0,4,"VacV controller beamline","   injector 1","       laser","          Vacuum","  ","        compressor 1",0.5554,0.01993,0.01993,1,0.9801]
[0,0,0,0,"timing beamline","   injector 1","       laser","        controls","  ","        compressor 2",0.8572,0.004981,0.004981,2,1.995]
[0.1,1,1,1,"other controls beamline","   injector 1","       laser","        controls","  ","          main linac",4.148,0.08023,0.08023,2,1.92]
[0,0,0,0,"Electrical - >0.5 beamline","   injector 1","       laser","        AC power","  ","              SASE 1",0.2881,1.498,0.1437,2,1.856]
[0,0,0,0,"Electrical - .05<<0.5 beamline","   injector 1","       laser","        AC power","  ","              SASE 2",0.4207,0.1084,0.1084,2,1.892]
[0,0,0,0,"LLRF cavity","   injector 1","      RF gun","        controls","  ","           all users",0,0,0,0,0]
[0,0,0,0,"coupler interlock sensors coupler","   injector 1","      RF gun","    RF structure","  ","% time down incl forced MD                 ",9.26]
[0,0,0,0,"coupler interlock electronics coupler","   injector 1","      RF gun","    RF structure","  ","% time fully up integrating lum or sched MD",86]
[0,0,0,0,"VacP coupler","   injector 1","      RF gun","    RF structure","  ","% time scheduled maintenance               ",4.68]
[0.2,1,0,1,"VacP power supply coupler","   injector 1","      RF gun","    RF structure","  ","% time integrating lum                     ",79.2]
[0,0,0,0,"VacP beamline","   injector 1","      RF gun","          Vacuum","  ","% time scheduled MD                        ",6.79]
[0,0,1,1,"VacP power supply beamline","   injector 1","      RF gun","          Vacuum","  ","% time actual opportunistic MD             ",1.21]
[0.7,2,1,2,"Modulators klystron","   injector 1","      RF gun","RF power sources","  ","% time useless down                        ",8.04]
[0.3,1,0,1,"Pulse transformers klystron","   injector 1","      RF gun","RF power sources"]
[2.2,4,1,4,"Klystrons klystron","   injector 1","      RF gun","RF power sources"]
[0.1,1,1,1,"klys pre-amp klystron","   injector 1","      RF gun","RF power sources"]
[0,0,1,0,"VacG/Ctrl klystron","   injector 1","      RF gun","RF power sources"]
[0,0,0,0,"VacP klystron","   injector 1","      RF gun","RF power sources"]
[0,0,0,0,"spare klystron klystron","   injector 1","      RF gun","RF power sources"]
[0.4,2,0,2,"VacP power supply klystron","   injector 1","      RF gun","RF power sources"]
[0.2,1,0,1,"LLRF klystron","   injector 1","      RF gun","        controls"]
[0.3,2,0,2,"timing klystron","   injector 1","      RF gun","        controls"]
[1.4,7,1,7,"other controls klystron","   injector 1","      RF gun","        controls"]
[0.4,1,0,1,"Electrical - >0.5 klystron","   injector 1","      RF gun","        AC power"]
[0.2,1,0,1,"Electrical - .05<<0.5 klystron","   injector 1","      RF gun","        AC power"]
[0,0,0,0,"Corrs - can't tune around beamline","   injector 1","      RF gun","         Magnets"]
[0,0,0,0,"PS Corrs can't tune around beamline","   injector 1","      RF gun","PS + controllers"]
[0.3,2,0,2,"PS controller - corr can't tune around beamline","   injector 1","      RF gun","PS + controllers"]
[2.4,3,0,3,"Vac Mech device beamline","   injector 1","      RF gun","          Vacuum"]
[0,0,0,0,"VacP beamline","   injector 1","      RF gun","          Vacuum"]
[0,0,2,2,"VacP power supply beamline","   injector 1","      RF gun","          Vacuum"]
[0,0,0,0,"VacV beamline","   injector 1","      RF gun","          Vacuum"]
[1.2,5,1,5,"VacV controller beamline","   injector 1","      RF gun","          Vacuum"]
[0,0,1,1,"BPMs diagnostic","   injector 1","      RF gun","      Diagnostic"]
[3.8,5,0,5,"Quads beamline","   injector 1","       linac","         Magnets"]
[0,0,0,0,"Quads SC beamline","   injector 1","       linac","         Magnets"]
[0,0,0,0,"Quad/Sext trims beamline","   injector 1","       linac","         Magnets"]
[0,0,0,16,"quad or corr beamline","   injector 1","       linac","         Magnets"]
[0,0,0,0,"Corrs - can tune around beamline","   injector 1","       linac","         Magnets"]
[0,0,0,0,"Wigglers beamline","   injector 1","       linac","         Magnets"]
[0,0,0,0,"Kickers beamline","   injector 1","       linac","         Magnets"]
[0,0,0,0,"Kicker pulser beamline","   injector 1","       linac","PS + controllers"]
[2,6,2,6,"Power supplies SC quad beamline","   injector 1","       linac","PS + controllers"]
[2.7,16,0,16,"Power supplies strings beamline","   injector 1","       linac","PS + controllers"]
[0.2,5,1,5,"PS Corrs can tune around beamline","   injector 1","       linac","PS + controllers"]
[0,0,0,2,"Power supplies Trims beamline","   injector 1","       linac","PS + controllers"]
[0.2,1,0,1,"PS controller SC quad beamline","   injector 1","       linac","PS + controllers"]
[0.9,9,1,9,"PS controller string beamline","   injector 1","       linac","PS + controllers"]
[0.5,11,6,11,"PS controller - corr can tune around beamline","   injector 1","       linac","PS + controllers"]
[0.6,4,0,4,"Flow Switch - quads beamline","   injector 1","       linac","    Water system"]
[0,0,0,0,"cryo vac enclosure cryo segment","   injector 1","       linac","            Cryo"]
[4.7,6,0,6,"Vac Mech device beamline","   injector 1","       linac","          Vacuum"]
[0,0,0,0,"VacP beamline","   injector 1","       linac","          Vacuum"]
[0,0,2,16,"VacP power supply beamline","   injector 1","       linac","          Vacuum"]
[0.4,1,1,1,"VacV beamline","   injector 1","       linac","          Vacuum"]
[1.2,5,1,5,"VacV controller beamline","   injector 1","       linac","          Vacuum"]
[0,0,5,24,"BPMs diagnostic","   injector 1","       linac","      Diagnostic"]
[0,0,1,7,"wire scanners diagnostic","   injector 1","       linac","      Diagnostic"]
[0,0,0,0,"Kicker diagnostic","   injector 1","       linac","      Diagnostic"]
[0,0,0,0,"Kicker pulser diagnostic","   injector 1","       linac","      Diagnostic"]
[0.1,1,0,1,"controls backbone sector","   injector 1","       linac","        controls"]
[0.2,2,0,2,"timing sector","   injector 1","       linac","        controls"]
[2.7,26,2,26,"local backbone sector","   injector 1","       linac","        controls"]
[0.4,4,0,4,"Controls PPS region","   injector 1","       linac","        controls"]
[2.2,23,5,23,"MPS & FastFdbk region","   injector 1","       linac","        controls"]
[3.5,13,1,13,"Electrical - .05<<0.5 Utility power","   injector 1","       linac","        AC power"]
[0,0,0,0,"Cavities cavity","   injector 1","       linac","    RF structure"]
[0,0,0,0,"Cavities cavity","   injector 1","       linac","    RF structure"]
[0,0,0,1,"Cavity tuner cavity","   injector 1","       linac","    RF structure"]
[0,0,0,3,"Cavity piezo tuner cavity","   injector 1","       linac","    RF structure"]
[0,0,2,8,"LLRF cavity","   injector 1","       linac","        controls"]
[0,0,0,0,"power coupler coupler","   injector 1","       linac","    RF structure"]
[0,0,0,0,"power coupler coupler","   injector 1","       linac","    RF structure"]
[0,0,0,0,"power coupler disc coupler","   injector 1","       linac","    RF structure"]
[0,0,0,0,"coupler interlock sensors coupler","   injector 1","       linac","    RF structure"]
[0.2,1,0,1,"coupler interlock electronics coupler","   injector 1","       linac","    RF structure"]
[0,0,0,0,"VacP coupler","   injector 1","       linac","    RF structure"]
[0.8,5,0,5,"VacP power supply coupler","   injector 1","       linac","    RF structure"]
[0,0,0,0,"VacP beamline","   injector 1","       linac","          Vacuum"]
[0,0,0,1,"VacP power supply beamline","   injector 1","       linac","          Vacuum"]
[1.4,2,1,2,"insulating vacuumP cryo string","   injector 1","       linac","            Cryo"]
[0.3,1,0,1,"cryo JT valve cryo string","   injector 1","       linac","            Cryo"]
[0,0,0,0,"VacV beamline","   injector 1","       linac","          Vacuum"]
[0,0,0,0,"VacV controller beamline","   injector 1","       linac","          Vacuum"]
[0,0,0,0,"cryo vac enclosure cryo segment","   injector 1","       linac","            Cryo"]
[1.8,5,1,5,"Modulators klystron","   injector 1","       linac","RF power sources"]
[0,0,0,0,"pulse cables klystron","   injector 1","       linac","RF power sources"]
[0,0,0,0,"Pulse transformers klystron","   injector 1","       linac","RF power sources"]
[0,0,0,0,"Klystrons klystron","   injector 1","       linac","RF power sources"]
[0,0,0,0,"Flow Switch klystron","   injector 1","       linac","    Water system"]
[0.2,2,0,2,"klys pre-amp klystron","   injector 1","       linac","RF power sources"]
[0.2,1,0,1,"VacG/Ctrl klystron","   injector 1","       linac","RF power sources"]
[0,0,0,0,"VacP klystron","   injector 1","       linac","RF power sources"]
[0,0,0,0,"spare klystron klystron","   injector 1","       linac","RF power sources"]
[0.1,1,0,1,"VacP power supply klystron","   injector 1","       linac","RF power sources"]
[0.2,1,0,1,"LLRF klystron","   injector 1","       linac","        controls"]
[1.1,5,0,5,"timing klystron","   injector 1","       linac","        controls"]
[0.2,1,0,1,"other controls klystron","   injector 1","       linac","        controls"]
[4.9,7,0,7,"Quads beamline"," compressor 1","            ","         Magnets"]
[0,0,0,0,"Quads SC beamline"," compressor 1","            ","         Magnets"]
[0,0,0,0,"Quad/Sext trims beamline"," compressor 1","            ","         Magnets"]
[0,0,0,21,"quad or corr beamline"," compressor 1","            ","         Magnets"]
[0,0,0,0,"Corrs - can tune around beamline"," compressor 1","            ","         Magnets"]
[0,0,0,0,"Wigglers beamline"," compressor 1","            ","         Magnets"]
[0,0,0,0,"Kickers beamline"," compressor 1","            ","         Magnets"]
[0,0,0,0,"Kicker pulser beamline"," compressor 1","            ","PS + controllers"]
[11.8,30,7,30,"Power supplies SC quad beamline"," compressor 1","            ","PS + controllers"]
[1.7,10,2,10,"Power supplies strings beamline"," compressor 1","            ","PS + controllers"]
[0.5,12,0,12,"PS Corrs can tune around beamline"," compressor 1","            ","PS + controllers"]
[0,0,0,1,"Power supplies Trims beamline"," compressor 1","            ","PS + controllers"]
[0.8,4,0,4,"PS controller SC quad beamline"," compressor 1","            ","PS + controllers"]
[0.5,7,1,7,"PS controller string beamline"," compressor 1","            ","PS + controllers"]
[0.4,9,2,9,"PS controller - corr can tune around beamline"," compressor 1","            ","PS + controllers"]
[0.4,3,0,3,"Flow Switch - quads beamline"," compressor 1","            ","    Water system"]
[0,0,0,0,"cryo vac enclosure cryo segment"," compressor 1","            ","            Cryo"]
[18.3,26,2,26,"Vac Mech device beamline"," compressor 1","            ","          Vacuum"]
[0,0,0,0,"VacP beamline"," compressor 1","            ","          Vacuum"]
[0,0,0,6,"VacP power supply beamline"," compressor 1","            ","          Vacuum"]
[0.5,1,0,1,"VacV beamline"," compressor 1","            ","          Vacuum"]
[1,4,0,4,"VacV controller beamline"," compressor 1","            ","          Vacuum"]
[0,0,6,46,"BPMs diagnostic"," compressor 1","            ","      Diagnostic"]
[0,0,2,20,"wire scanners diagnostic"," compressor 1","            ","      Diagnostic"]
[0,0,0,0,"Kicker diagnostic"," compressor 1","            ","      Diagnostic"]
[0,0,0,0,"Kicker pulser diagnostic"," compressor 1","            ","      Diagnostic"]
[0,0,0,0,"controls backbone sector"," compressor 1","            ","        controls"]
[0.1,1,0,1,"timing sector"," compressor 1","            ","        controls"]
[2.7,31,4,31,"local backbone sector"," compressor 1","            ","        controls"]
[0.3,3,1,3,"Controls PPS region"," compressor 1","            ","        controls"]
[2,25,8,25,"MPS & FastFdbk region"," compressor 1","            ","        controls"]
[2.9,12,2,12,"Electrical - .05<<0.5 Utility power"," compressor 1","            ","        AC power"]
[0,0,1,0,"Modulators klystron"," compressor 1","            ","      Diagnostic"]
[0,0,0,0,"Pulse transformers klystron"," compressor 1","            ","      Diagnostic"]
[0,0,0,1,"Klystrons klystron"," compressor 1","            ","      Diagnostic"]
[0,0,0,0,"klys pre-amp klystron"," compressor 1","            ","      Diagnostic"]
[0,0,0,1,"VacG/Ctrl klystron"," compressor 1","            ","      Diagnostic"]
[0,0,0,0,"VacP klystron"," compressor 1","            ","      Diagnostic"]
[0,0,0,0,"VacP power supply klystron"," compressor 1","            ","      Diagnostic"]
[0,0,0,0,"Cavities cavity"," compressor 1","       linac","    RF structure"]
[0,0,0,0,"Cavities cavity"," compressor 1","       linac","    RF structure"]
[0,0,0,5,"Cavity tuner cavity"," compressor 1","       linac","    RF structure"]
[0,0,0,8,"Cavity piezo tuner cavity"," compressor 1","       linac","    RF structure"]
[0,0,7,46,"LLRF cavity"," compressor 1","       linac","        controls"]
[0,0,0,1,"power coupler coupler"," compressor 1","       linac","    RF structure"]
[0.2,1,0,1,"power coupler coupler"," compressor 1","       linac","    RF structure"]
[0,0,0,2,"power coupler disc coupler"," compressor 1","       linac","    RF structure"]
[1.3,7,2,7,"coupler interlock sensors coupler"," compressor 1","       linac","    RF structure"]
[1.1,6,1,6,"coupler interlock electronics coupler"," compressor 1","       linac","    RF structure"]
[0,0,0,0,"VacP coupler"," compressor 1","       linac","    RF structure"]
[0.5,3,0,3,"VacP power supply coupler"," compressor 1","       linac","    RF structure"]
[0,0,0,0,"VacP beamline"," compressor 1","       linac","          Vacuum"]
[0,0,4,9,"VacP power supply beamline"," compressor 1","       linac","          Vacuum"]
[0,0,0,0,"insulating vacuumP cryo string"," compressor 1","       linac","            Cryo"]
[0,0,0,0,"cryo JT valve cryo string"," compressor 1","       linac","            Cryo"]
[0,0,0,0,"VacV beamline"," compressor 1","       linac","          Vacuum"]
[0.3,1,0,1,"VacV controller beamline"," compressor 1","       linac","          Vacuum"]
[0,0,0,0,"cryo vac enclosure cryo segment"," compressor 1","       linac","            Cryo"]
[0.3,1,1,1,"Modulators klystron"," compressor 1","       linac","RF power sources"]
[0,0,0,0,"pulse cables klystron"," compressor 1","       linac","RF power sources"]
[0.3,1,0,1,"Pulse transformers klystron"," compressor 1","       linac","RF power sources"]
[2.1,4,1,4,"Klystrons klystron"," compressor 1","       linac","RF power sources"]
[0,0,0,0,"Flow Switch klystron"," compressor 1","       linac","    Water system"]
[0.1,1,1,1,"klys pre-amp klystron"," compressor 1","       linac","RF power sources"]
[0,0,0,0,"VacG/Ctrl klystron"," compressor 1","       linac","RF power sources"]
[0,0,0,0,"VacP klystron"," compressor 1","       linac","RF power sources"]
[0,0,0,0,"spare klystron klystron"," compressor 1","       linac","RF power sources"]
[0.1,1,0,1,"VacP power supply klystron"," compressor 1","       linac","RF power sources"]
[0.1,1,0,1,"LLRF klystron"," compressor 1","       linac","        controls"]
[0,0,0,0,"timing klystron"," compressor 1","       linac","        controls"]
[0.5,3,0,3,"other controls klystron"," compressor 1","       linac","        controls"]
[2.4,3,1,3,"Quads beamline"," compressor 2","            ","         Magnets"]
[0,0,0,0,"Quads SC beamline"," compressor 2","            ","         Magnets"]
[0,0,0,0,"Quad/Sext trims beamline"," compressor 2","            ","         Magnets"]
[0,0,0,22,"quad or corr beamline"," compressor 2","            ","         Magnets"]
[0,0,0,0,"Corrs - can tune around beamline"," compressor 2","            ","         Magnets"]
[0,0,0,0,"Wigglers beamline"," compressor 2","            ","         Magnets"]
[0,0,0,0,"Kickers beamline"," compressor 2","            ","         Magnets"]
[0,0,0,0,"Kicker pulser beamline"," compressor 2","            ","PS + controllers"]
[32.9,80,11,80,"Power supplies SC quad beamline"," compressor 2","            ","PS + controllers"]
[2.1,12,0,12,"Power supplies strings beamline"," compressor 2","            ","PS + controllers"]
[0.4,9,0,9,"PS Corrs can tune around beamline"," compressor 2","            ","PS + controllers"]
[0,0,0,0,"Power supplies Trims beamline"," compressor 2","            ","PS + controllers"]
[0.6,4,3,4,"PS controller SC quad beamline"," compressor 2","            ","PS + controllers"]
[1.3,16,1,16,"PS controller string beamline"," compressor 2","            ","PS + controllers"]
[0.5,13,5,13,"PS controller - corr can tune around beamline"," compressor 2","            ","PS + controllers"]
[0.6,4,0,4,"Flow Switch - quads beamline"," compressor 2","            ","    Water system"]
[0,0,0,0,"cryo vac enclosure cryo segment"," compressor 2","            ","            Cryo"]
[9.2,14,2,14,"Vac Mech device beamline"," compressor 2","            ","          Vacuum"]
[0,0,0,0,"VacP beamline"," compressor 2","            ","          Vacuum"]
[0,0,3,8,"VacP power supply beamline"," compressor 2","            ","          Vacuum"]
[0.4,1,0,1,"VacV beamline"," compressor 2","            ","          Vacuum"]
[1,4,1,4,"VacV controller beamline"," compressor 2","            ","          Vacuum"]
[0,0,11,41,"BPMs diagnostic"," compressor 2","            ","      Diagnostic"]
[0,0,0,17,"wire scanners diagnostic"," compressor 2","            ","      Diagnostic"]
[0,0,0,0,"Kicker diagnostic"," compressor 2","            ","      Diagnostic"]
[0,0,0,0,"Kicker pulser diagnostic"," compressor 2","            ","      Diagnostic"]
[0.3,4,0,4,"controls backbone sector"," compressor 2","            ","        controls"]
[0,0,0,0,"timing sector"," compressor 2","            ","        controls"]
[3.2,39,2,39,"local backbone sector"," compressor 2","            ","        controls"]
[0.2,2,0,2,"Controls PPS region"," compressor 2","            ","        controls"]
[2.3,29,4,29,"MPS & FastFdbk region"," compressor 2","            ","        controls"]
[3.3,15,1,15,"Electrical - .05<<0.5 Utility power"," compressor 2","            ","        AC power"]
[0,0,1,0,"Modulators klystron"," compressor 2","            ","      Diagnostic"]
[0,0,0,1,"Pulse transformers klystron"," compressor 2","            ","      Diagnostic"]
[0,0,1,5,"Klystrons klystron"," compressor 2","            ","      Diagnostic"]
[0,0,1,1,"klys pre-amp klystron"," compressor 2","            ","      Diagnostic"]
[0,0,0,2,"VacG/Ctrl klystron"," compressor 2","            ","      Diagnostic"]
[0,0,0,0,"VacP klystron"," compressor 2","            ","      Diagnostic"]
[0,0,0,3,"VacP power supply klystron"," compressor 2","            ","      Diagnostic"]
[0,0,0,0,"Cavities cavity"," compressor 2","       linac","    RF structure"]
[0,0,0,0,"Cavities cavity"," compressor 2","       linac","    RF structure"]
[0,0,5,9,"Cavity tuner cavity"," compressor 2","       linac","    RF structure"]
[0,0,7,24,"Cavity piezo tuner cavity"," compressor 2","       linac","    RF structure"]
[0,0,22,151,"LLRF cavity"," compressor 2","       linac","        controls"]
[0,0,0,0,"power coupler coupler"," compressor 2","       linac","    RF structure"]
[0.4,2,0,2,"power coupler coupler"," compressor 2","       linac","    RF structure"]
[0,0,0,2,"power coupler disc coupler"," compressor 2","       linac","    RF structure"]
[2.1,13,3,13,"coupler interlock sensors coupler"," compressor 2","       linac","    RF structure"]
[2.3,15,1,15,"coupler interlock electronics coupler"," compressor 2","       linac","    RF structure"]
[0.5,1,0,1,"VacP coupler"," compressor 2","       linac","    RF structure"]
[1.7,10,2,10,"VacP power supply coupler"," compressor 2","       linac","    RF structure"]
[0,0,0,0,"VacP beamline"," compressor 2","       linac","          Vacuum"]
[0,0,2,14,"VacP power supply beamline"," compressor 2","       linac","          Vacuum"]
[2.3,3,1,3,"insulating vacuumP cryo string"," compressor 2","       linac","            Cryo"]
[0,0,0,0,"cryo JT valve cryo string"," compressor 2","       linac","            Cryo"]
[0,0,0,0,"VacV beamline"," compressor 2","       linac","          Vacuum"]
[0,0,0,0,"VacV controller beamline"," compressor 2","       linac","          Vacuum"]
[0,0,0,0,"cryo vac enclosure cryo segment"," compressor 2","       linac","            Cryo"]
[2.6,8,1,8,"Modulators klystron"," compressor 2","       linac","RF power sources"]
[0.7,1,0,1,"pulse cables klystron"," compressor 2","       linac","RF power sources"]
[1.4,3,0,3,"Pulse transformers klystron"," compressor 2","       linac","RF power sources"]
[6.3,12,2,12,"Klystrons klystron"," compressor 2","       linac","RF power sources"]
[0.2,2,0,2,"Flow Switch klystron"," compressor 2","       linac","    Water system"]
[0.4,5,1,5,"klys pre-amp klystron"," compressor 2","       linac","RF power sources"]
[1,6,1,6,"VacG/Ctrl klystron"," compressor 2","       linac","RF power sources"]
[0,0,0,0,"VacP klystron"," compressor 2","       linac","RF power sources"]
[0,0,0,0,"spare klystron klystron"," compressor 2","       linac","RF power sources"]
[0.9,6,1,6,"VacP power supply klystron"," compressor 2","       linac","RF power sources"]
[0.4,2,0,2,"LLRF klystron"," compressor 2","       linac","        controls"]
[0.3,2,1,2,"timing klystron"," compressor 2","       linac","        controls"]
[1.5,9,2,9,"other controls klystron"," compressor 2","       linac","        controls"]
[0,0,0,0,"Quads beamline","   main linac","            ","         Magnets"]
[0.3,2,1,2,"Quads SC beamline","   main linac","            ","         Magnets"]
[0,0,0,0,"Quad/Sext trims beamline","   main linac","            ","         Magnets"]
[0,0,0,87,"quad or corr beamline","   main linac","            ","         Magnets"]
[0,1,0,1,"Corrs - can tune around beamline","   main linac","            ","         Magnets"]
[0,0,0,0,"Wigglers beamline","   main linac","            ","         Magnets"]
[0,0,0,0,"Kickers beamline","   main linac","            ","         Magnets"]
[0,0,0,0,"Kicker pulser beamline","   main linac","            ","PS + controllers"]
[277.2,683,116,683,"Power supplies SC quad beamline","   main linac","            ","PS + controllers"]
[0,0,0,0,"Power supplies strings beamline","   main linac","            ","PS + controllers"]
[1.4,38,5,38,"PS Corrs can tune around beamline","   main linac","            ","PS + controllers"]
[0,0,0,0,"Power supplies Trims beamline","   main linac","            ","PS + controllers"]
[9.8,59,4,59,"PS controller SC quad beamline","   main linac","            ","PS + controllers"]
[0,0,0,0,"PS controller string beamline","   main linac","            ","PS + controllers"]
[1.8,46,4,46,"PS controller - corr can tune around beamline","   main linac","            ","PS + controllers"]
[0,0,0,0,"Flow Switch - quads beamline","   main linac","            ","    Water system"]
[0,0,0,0,"cryo vac enclosure cryo segment","   main linac","            ","            Cryo"]
[0,0,0,0,"Vac Mech device beamline","   main linac","            ","          Vacuum"]
[0,0,0,0,"VacP beamline","   main linac","            ","          Vacuum"]
[0,0,0,0,"VacP power supply beamline","   main linac","            ","          Vacuum"]
[0,0,0,0,"VacV beamline","   main linac","            ","          Vacuum"]
[0,0,0,0,"VacV controller beamline","   main linac","            ","          Vacuum"]
[0,0,21,148,"BPMs diagnostic","   main linac","            ","      Diagnostic"]
[0,0,0,0,"wire scanners diagnostic","   main linac","            ","      Diagnostic"]
[0,0,0,0,"Kicker diagnostic","   main linac","            ","      Diagnostic"]
[0,0,0,0,"Kicker pulser diagnostic","   main linac","            ","      Diagnostic"]
[0.3,4,0,4,"controls backbone sector","   main linac","            ","        controls"]
[0.6,8,1,8,"timing sector","   main linac","            ","        controls"]
[11.2,150,25,150,"local backbone sector","   main linac","            ","        controls"]
[0.5,6,0,6,"Controls PPS region","   main linac","            ","        controls"]
[2,26,8,26,"MPS & FastFdbk region","   main linac","            ","        controls"]
[17.7,78,15,78,"Electrical - .05<<0.5 Utility power","   main linac","            ","        AC power"]
[0,0,0,3,"Cavities cavity","   main linac",0,"    RF structure"]
[0,0,1,1,"Cavities cavity","   main linac",0,"    RF structure"]
[0,0,12,106,"Cavity tuner cavity","   main linac",0,"    RF structure"]
[0,0,30,218,"Cavity piezo tuner cavity","   main linac",0,"    RF structure"]
[0,0,172,1087,"LLRF cavity","   main linac",0,"        controls"]
[0,0,4,11,"power coupler coupler","   main linac",0,"    RF structure"]
[1.3,6,1,14,"power coupler coupler","   main linac",0,"    RF structure"]
[0,0,0,25,"power coupler disc coupler","   main linac",0,"    RF structure"]
[5.4,28,18,124,"coupler interlock sensors coupler","   main linac",0,"    RF structure"]
[3.3,18,16,99,"coupler interlock electronics coupler","   main linac",0,"    RF structure"]
[0,0,0,0,"VacP coupler","   main linac",0,"    RF structure"]
[5.6,33,21,137,"VacP power supply coupler","   main linac",0,"    RF structure"]
[0,0,0,2,"VacP beamline","   main linac",0,"          Vacuum"]
[0,0,26,133,"VacP power supply beamline","   main linac",0,"          Vacuum"]
[7.9,11,2,11,"insulating vacuumP cryo string","   main linac",0,"            Cryo"]
[1,5,1,5,"cryo JT valve cryo string","   main linac",0,"            Cryo"]
[0.5,1,0,1,"VacV beamline","   main linac",0,"          Vacuum"]
[1.8,9,2,9,"VacV controller beamline","   main linac",0,"          Vacuum"]
[0,0,0,0,"cryo vac enclosure cryo segment","   main linac",0,"            Cryo"]
[1.8,7,12,69,"Modulators klystron","   main linac",0,"RF power sources"]
[1.6,3,4,19,"pulse cables klystron","   main linac",0,"RF power sources"]
[0.5,1,5,8,"Pulse transformers klystron","   main linac",0,"RF power sources"]
[2.9,8,11,76,"Klystrons klystron","   main linac",0,"RF power sources"]
[0.1,1,2,12,"Flow Switch klystron","   main linac",0,"    Water system"]
[0.5,7,6,36,"klys pre-amp klystron","   main linac",0,"RF power sources"]
[0.5,3,3,33,"VacG/Ctrl klystron","   main linac",0,"RF power sources"]
[0,0,0,0,"VacP klystron","   main linac",0,"RF power sources"]
[0,0,0,0,"spare klystron klystron","   main linac",0,"RF power sources"]
[1.9,10,5,37,"VacP power supply klystron","   main linac",0,"RF power sources"]
[1.4,6,6,33,"LLRF klystron","   main linac",0,"        controls"]
[1.3,8,1,38,"timing klystron","   main linac",0,"        controls"]
[4,21,17,87,"other controls klystron","   main linac",0,"        controls"]
[13,18,5,18,"Quads beamline","   main linac",0,"         Magnets"]
[0,0,0,0,"Quads SC beamline","   main linac",0,"         Magnets"]
[0,0,0,0,"Quad/Sext trims beamline","   main linac",0,"         Magnets"]
[0,0,0,89,"quad or corr beamline","   main linac",0,"         Magnets"]
[0.2,5,0,5,"Corrs - can tune around beamline","   main linac",0,"         Magnets"]
[0,0,0,0,"Wigglers beamline","   main linac",0,"         Magnets"]
[0.4,2,4,25,"Kickers beamline","   main linac",0,"         Magnets"]
[4,17,33,246,"Kicker pulser beamline","   main linac",0,"PS + controllers"]
[0,0,2,11,"Kickers beamline","   main linac",0,"         Magnets"]
[5.6,24,44,258,"Kicker pulser beamline","   main linac",0,"PS + controllers"]
[4.5,29,5,29,"Power supplies strings beamline","   main linac",0,"PS + controllers"]
[1.1,29,6,29,"PS Corrs can tune around beamline","   main linac",0,"PS + controllers"]
[0,0,3,10,"Power supplies Trims beamline","   main linac",0,"PS + controllers"]
[2,28,6,28,"PS controller string beamline","   main linac",0,"PS + controllers"]
[2.1,55,12,55,"PS controller - corr can tune around beamline","   main linac",0,"PS + controllers"]
[3.4,21,6,21,"Flow Switch - quads beamline","   main linac",0,"    Water system"]
[0,0,0,0,"cryo vac enclosure cryo segment","   main linac",0,"            Cryo"]
[0,0,2,0,"Vac Mech device beamline","   main linac",0,"          Vacuum"]
[0,0,0,5,"VacP beamline","   main linac",0,"          Vacuum"]
[0,0,5,60,"VacP power supply beamline","   main linac",0,"          Vacuum"]
[0.8,2,1,2,"VacV beamline","   main linac",0,"          Vacuum"]
[3,12,0,12,"VacV controller beamline","   main linac",0,"          Vacuum"]
[0,0,15,101,"BPMs diagnostic","   main linac",0,"      Diagnostic"]
[0,0,0,0,"wire scanners diagnostic","   main linac",0,"      Diagnostic"]
[0,0,0,0,"Kicker diagnostic","   main linac",0,"      Diagnostic"]
[0,0,0,0,"Kicker pulser diagnostic","   main linac",0,"      Diagnostic"]
[0.1,2,1,2,"controls backbone sector","   main linac",0,"        controls"]
[0.1,1,0,1,"timing sector","   main linac",0,"        controls"]
[2,25,3,25,"local backbone sector","   main linac",0,"        controls"]
[0.5,6,0,6,"Controls PPS region","   main linac",0,"        controls"]
[3,41,3,41,"MPS & FastFdbk region","   main linac",0,"        controls"]
[2.9,12,3,12,"Electrical - .05<<0.5 Utility power","   main linac",0,"        AC power"]
[8.8,17,4,17,"Quads beamline","       SASE 1",0,"         Magnets"]
[0,0,0,0,"Quads SC beamline","       SASE 1",0,"         Magnets"]
[0,0,1,0,"Quad/Sext trims beamline","       SASE 1",0,"         Magnets"]
[0,0,0,153,"quad or corr beamline","       SASE 1",0,"         Magnets"]
[0.1,4,0,4,"Corrs - can tune around beamline","       SASE 1",0,"         Magnets"]
[0,0,11,74,"Undulator movers beamline","       SASE 1",0,"         Magnets"]
[0,0,0,0,"Kickers beamline","       SASE 1",0,"         Magnets"]
[0,0,0,0,"Kicker pulser beamline","       SASE 1",0,"PS + controllers"]
[3.2,25,7,25,"Power supplies strings beamline","       SASE 1",0,"PS + controllers"]
[2,57,10,57,"PS Corrs can tune around beamline","       SASE 1",0,"PS + controllers"]
[0,0,0,4,"Power supplies Trims beamline","       SASE 1",0,"PS + controllers"]
[1.2,17,2,17,"PS controller string beamline","       SASE 1",0,"PS + controllers"]
[3.2,92,15,92,"PS controller - corr can tune around beamline","       SASE 1",0,"PS + controllers"]
[4,26,3,26,"Flow Switch - quads beamline","       SASE 1",0,"    Water system"]
[0,0,0,0,"cryo vac enclosure cryo segment","       SASE 1",0,"            Cryo"]
[0,0,0,0,"Vac Mech device beamline","       SASE 1",0,"          Vacuum"]
[0,0,0,6,"VacP beamline","       SASE 1",0,"          Vacuum"]
[0,0,27,137,"VacP power supply beamline","       SASE 1",0,"          Vacuum"]
[0.3,1,0,1,"VacV beamline","       SASE 1",0,"          Vacuum"]
[0.6,3,0,3,"VacV controller beamline","       SASE 1",0,"          Vacuum"]
[0,0,27,168,"BPMs diagnostic","       SASE 1",0,"      Diagnostic"]
[0,0,0,0,"wire scanners diagnostic","       SASE 1",0,"      Diagnostic"]
[0,0,0,0,"Kicker diagnostic","       SASE 1",0,"      Diagnostic"]
[0,0,0,0,"Kicker pulser diagnostic","       SASE 1",0,"      Diagnostic"]
[0.1,1,0,1,"controls backbone sector","       SASE 1",0,"        controls"]
[0,0,0,0,"timing sector","       SASE 1",0,"        controls"]
[1.7,26,5,26,"local backbone sector","       SASE 1",0,"        controls"]
[0.1,1,0,1,"Controls PPS region","       SASE 1",0,"        controls"]
[1.6,22,2,22,"MPS & FastFdbk region","       SASE 1",0,"        controls"]
[1.9,10,1,10,"Electrical - .05<<0.5 Utility power","       SASE 1",0,"        AC power"]
[14.8,25,6,25,"Quads beamline","       SASE 2",0,"         Magnets"]
[0,0,0,0,"Quads SC beamline","       SASE 2",0,"         Magnets"]
[0,0,0,0,"Quad/Sext trims beamline","       SASE 2",0,"         Magnets"]
[0,0,0,166,"quad or corr beamline","       SASE 2",0,"         Magnets"]
[0.1,3,1,3,"Corrs - can tune around beamline","       SASE 2",0,"         Magnets"]
[0,0,8,69,"Undulator movers beamline","       SASE 2",0,"         Magnets"]
[0,0,0,0,"Kickers beamline","       SASE 2",0,"         Magnets"]
[0,0,0,0,"Kicker pulser beamline","       SASE 2",0,"PS + controllers"]
[5.5,40,7,40,"Power supplies strings beamline","       SASE 2",0,"PS + controllers"]
[2.3,68,9,68,"PS Corrs can tune around beamline","       SASE 2",0,"PS + controllers"]
[0,0,0,5,"Power supplies Trims beamline","       SASE 2",0,"PS + controllers"]
[2.1,31,6,31,"PS controller string beamline","       SASE 2",0,"PS + controllers"]
[3.2,95,11,95,"PS controller - corr can tune around beamline","       SASE 2",0,"PS + controllers"]
[4.8,27,5,27,"Flow Switch - quads beamline","       SASE 2",0,"    Water system"]
[0,0,0,0,"cryo vac enclosure cryo segment","       SASE 2",0,"            Cryo"]
[0,0,0,0,"Vac Mech device beamline","       SASE 2",0,"          Vacuum"]
[0,0,0,0,"VacP beamline","       SASE 2",0,"          Vacuum"]
[0,0,15,121,"VacP power supply beamline","       SASE 2",0,"          Vacuum"]
[1.6,4,0,4,"VacV beamline","       SASE 2",0,"          Vacuum"]
[1.5,8,2,8,"VacV controller beamline","       SASE 2",0,"          Vacuum"]
[0,0,34,207,"BPMs diagnostic","       SASE 2",0,"      Diagnostic"]
[0,0,0,0,"wire scanners diagnostic","       SASE 2",0,"      Diagnostic"]
[0,0,0,0,"Kicker diagnostic","       SASE 2",0,"      Diagnostic"]
[0,0,0,0,"Kicker pulser diagnostic","       SASE 2",0,"      Diagnostic"]
[0.1,1,0,1,"controls backbone sector","       SASE 2",0,"        controls"]
[0.1,1,0,1,"timing sector","       SASE 2",0,"        controls"]
[2,29,8,29,"local backbone sector","       SASE 2",0,"        controls"]
[0.2,3,0,3,"Controls PPS region","       SASE 2",0,"        controls"]
[1.3,19,1,19,"MPS & FastFdbk region","       SASE 2",0,"        controls"]
[2.5,12,3,12,"Electrical - .05<<0.5 Utility power","       SASE 2",0,"        AC power"]
[131.4,153,23,153,"cryo plant beamline","  Cryo plants","            ","          lumped"]
[69.9,78,13,78,"site power beamline","   Site power","            ","          lumped"]
[23.8,54,10,54,"Controls sitewide beamline","Global controls","            ","          lumped"]
[24.9,57,13,57,"Central Water beamline","Central Water","            ","          lumped"]
[1.4,0,0,0,"schedMaintn","    all users","            ","      schedMaint"]