{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":136,"n_cols":18,"rows_kept":136,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Last Revised 7/29/04 by John Kaminski"]
[]
["                                                                                                                             MASTER FOR MACHINE SHOP",{"$nulls":5},"                               LEPP MACHINE SHOP MASTER LOG "]
[]
["Submitted By","Account","Shop Job#","Date Sub","Date Req","Part#","Job Description or Part Name","Print #","Mat.","Qty","Time/Pc","Est. Time","Machine Tool","Prority","Machinist","Date Ass","Status","Notes"]
["rongli g","erl",3,null,null,null,"erl injector cavity",{"$nulls":10},"resume august"]
[{"$nulls":5},1,"power coupler block","7102-002-02","niobium",1,50,50,"mill",{"$nulls":4},"hold niobium"]
[{"$nulls":5},2,"female center half cell         chc","7102-002-02","niobium",2,12,24,"cnc-mill",{"$nulls":4},"hold"]
[{"$nulls":5},3,"male center half cell            chc","7102-002-02","niobium",2,12,24,"cnc-mill",{"$nulls":4},"hold"]
[{"$nulls":5},4,"center half cell                     ehc","7102-002-03","niobium",2,12,24,"cnc-mill",{"$nulls":4},"hold"]
[{"$nulls":5},5,"large beam tube stub","7102-002-04","niobium",2,8,16,"cnc-mill",{"$nulls":4},"hold"]
[{"$nulls":5},6,"large beam pipe end ring","7102-002-05","niobium",2,8,16,"lathe",{"$nulls":4},"hold"]
[{"$nulls":5},7,"rf probe pipe","7102-002-05","niobium",2,2,4,"lathe",{"$nulls":4},"hold"]
[{"$nulls":5},8,"1 1/3 rf probe flange","7102-002-05","316L",2,8,16,"lathe",{"$nulls":4},"hold"]
[{"$nulls":5},9,"rf probe port plug","7102-002-05","316L",2,0,0,"lathe",{"$nulls":4},"hold"]
[{"$nulls":5},12,"large beam pipe","7102-002-06","niobium",2,12,24,"lathe",{"$nulls":4},"waiting for print changes"]
[{"$nulls":5},13,"6 3/4 large beam pipe flange","7102-002-06","316L",1,10,10,"lathe",{"$nulls":4},"waiting for print changes"]
[{"$nulls":5},14,"large beam pipe plug","7102-002-06","316L",1,8,8,"lathe",{"$nulls":4},"hold"]
[{"$nulls":5},17,"small beam pipe","7102-002-07","niobium",2,6,12,"lathe",{"$nulls":4},"waiting for print changes"]
[{"$nulls":5},18,"6 inch beam pipe flange","7102-002-07","316L",1,12,12,"lathe",{"$nulls":4},"waiting for print changes"]
[{"$nulls":5},19,"small beam pipe plug","7102-002-07","316L",1,0,0,"lathe",{"$nulls":4},"hold"]
[{"$nulls":5},21,"input power coupler pipe","7102-002-08","niobium",4,10,40,"lathe",{"$nulls":4},"hold"]
[{"$nulls":5},22,"4 1/2 inch coupler flange","7102-002-08","316L",2,10,20,"lathe",{"$nulls":4},"hold"]
[{"$nulls":5},23,"input coupler plug","7102-002-08","316L",1,5,5,"lathe",{"$nulls":4},"hold"]
[{"$nulls":6},"ehc guillotine gage","7102-001-05",null,2]
[{"$nulls":6},"chc guillotine gage","7102-001-01",null,2]
[null,null,null,"2004-07-21",null,null,"large beam tube assy-2",{"$nulls":10},"2 assy"]
[{"$nulls":6},"6 3/4 cf rotatable ring","7102-002-0103","ss",2,5,10,"lathe"]
[{"$nulls":6},"6 3/4 cf flange ring","7102-002-0105","ss",2,5,10,"lathe/mill"]
[{"$nulls":6},"large beam tube flange","7102-002-010101","316LN",2,10,20,"lathe/mill"]
[{"$nulls":6},"large beam tube","7102-002-010102","niobium",2,10,20,"roll/lathe"]
[{"$nulls":6},"brazing plug","7102-002,IT. 14",6061,1,5,5,"lathe"]
[{"$nulls":6},"swagging plug",null,7075,1,3,3,"lathe"]
[{"$nulls":6},"stripper",null,7075,1,3,3,"lathe"]
[{"$nulls":6},"roll nb erl injector cavity beam tube ",null,"niobium",2,3,6,"roll/mill"]
[{"$nulls":11},305,"est time"]
[]
["karl s","erl",20,"2004-03-30",null,null,"energy recover linac"]
[null,null,20,"2004-05-26",null,null,"erl gun hv insulator"]
[{"$nulls":6},"male die",null,7075,1,8,8,"lathe"]
[{"$nulls":6},"female die",null,7075,1,8,8,"lathe"]
[{"$nulls":6},"kover braze ring",null,"         kovar",12,3,36,"press/trim"]
[{"$nulls":6},"6 inch rogowski elecdrode",null,"ss/titanium",null,null,null,"cnc-lathe"]
[{"$nulls":11},52,"est time"]
[]
["shop",{"$nulls":5},"building shelving stock area"]
[{"$nulls":6},"reorganized vidmar"]
[{"$nulls":6},"make small parallel"]
[{"$nulls":6},"spacer on 100 ton press",{"$nulls":10},"replace"]
[{"$nulls":6},"move punch press"]
[]
["john b","s-ring",16,"2004-05-27",null,null,"ferrite groud fault monitor for cesr","19 assy",{"$nulls":9},"1 assy done"]
[{"$nulls":5},1,"e-block","6042-034-02","g-10",19,8,144,"mill",null,"rm","2004-07-16","hold"]
[{"$nulls":5},2,"e-block bar","6042-034-02","g-10",19,3,57,"mill"]
[{"$nulls":5},7,"ferrite-long","6042-034-01","ferrite",36,1,36,"surface grinder",{"$nulls":4},"moo"]
[{"$nulls":5},8,"ferrite-short","6042-034-01","ferrite",36,1,36,"surface grinder",{"$nulls":4},"moo"]
[{"$nulls":5},10,"ferrite-long splithalf","6042-034-01","ferrite",36,1,36,"surface grinder",{"$nulls":4},"moo"]
[{"$nulls":11},309,"est time",{"$nulls":4},"14 hrs/assy"]
[]
[]
["mark p","cs-ring",30,"2004-05-17",null,null,"g-line skew quad","7 assy",{"$nulls":8},"6 assy"," 1 assy done"]
[{"$nulls":5},7,"pole","6019-210-04","steel",28,6,168,"mill",null,"tr/na","2004-07-12","done"]
[{"$nulls":5},8,"plate","6019-210-05","g-10",28,3,84,"mill"]
[{"$nulls":5},9,"bracket","6019-210-05","ss",56,1,56,"mill"]
[null,null,null," ",null,10,"spacer","6019-210-05","g-10",56,2,112,"mill",null,"austin","2004-07-10","done"]
[{"$nulls":5},11,"bottom plate","6019-210-05","ss",56,1,56,"mill",null,"austin","2004-07-10","done"]
[{"$nulls":5},12,"support bar","6019-210-06",6061,56,1,56,"mill",null,"austin","2004-07-10","done"]
[{"$nulls":5},13,"terminal block 1","6019-210-06","cu",84,1,84,"mill"]
[{"$nulls":5},14,"terminal block 2","6019-210-06","cu",56,1,56,"mill"]
[{"$nulls":5},15,"connector","6019-210-06",6061,28,1,28,"mill"]
[{"$nulls":5},34,"support plate-1","6019-210-07",6061,14,4,56,"cnc-mill",null,"hh","2004-07-01","14 done"]
[{"$nulls":5},35,"support plate-2","6019-210-08",6061,14,3,42,"cnc-mill",null,"tr","2004-07-01","14 done"]
[{"$nulls":5},36,"clamp","6019-210-09",6061,28,2,56,"mill"]
[{"$nulls":5},39,"support plate-3","6019-210-09",6061,7,2,14,"mill"]
[{"$nulls":5},37,"level plate","6019-210-10",6061,7,2,14,"mill",null,"tr","2004-07-08","6 done"]
[{"$nulls":5},38,"push/pull block","6019-210-10",6061,14,2,28,"mill"]
[{"$nulls":5},40,"screw modification","6019-210-10","ss",28,0.25,7,"lathe"]
[{"$nulls":11},917,"est time",{"$nulls":4},"131 hrs/assy"]
[]
[]
["mark p","cs-ring",30,null,null,null,"sextupole",null,null,24,null,null,"mill",{"$nulls":4},"print not issued"]
[{"$nulls":6},"thread rod",null,"ss",15,5,45,"lathe",null,null,null,"4done","prints not issued"]
[{"$nulls":4},"2004-07-22",null,"nose piece",null,1006,"8+10",3,30,"cnc-mill",null,"na","2004-07-26"]
[{"$nulls":6},"trim end packs",null,"lamination","8+10",4,32,"cnc-mill",null,"hh","2004-07-28"]
[{"$nulls":6},"fit nose piece to end packs",null,null,8,3,24,"mill"]
[{"$nulls":6},"cut replacement lamanations",null,"lamination",7,1.5,12,"cnc-mill",null,"hh","2004-07-27","done"]
[{"$nulls":6},"spacer","6041-158-02",1006,4,12,48,"mill",null,"rs","2004-07-26"]
[{"$nulls":6},"alinement rod",null,"ss",8,0.5,4,"lathe",{"$nulls":4},"moo"]
[{"$nulls":6},"lifting fixture",{"$nulls":5},"mill",{"$nulls":4},"prints not issued"]
["volker c",null,null,null,"2004-07-21",null,"scintillator",null,null,6,2,12,"mill",null,"rm","2004-07-26","done"]
[{"$nulls":4},"2004-07-21",null,"light guide",null,null,6,3,18,"cnc-mill",null,"sm","2004-07-26","done"]
[{"$nulls":6},"frame for detector",null,6061,{"$nulls":8},"prints not issued"]
[null,null,null,"2004-07-27",null,14,"coil retainer","6041-158-01","g-10",4,3,12,"cnc-mill",null,"ds","2004-07-28"]
[null,null,null,"2004-07-27",null,17,"coil support","6041-158-01","g-10",4,3,12,"cnc-mill",null,"ds","2004-07-28"]
["yulin l",null,null,"2004-07-26","2004-07-29",null,"stiffener for q3w chamber",null,"cu",2,7,14,"mill",null,"rm","2004-07-28","done"]
[{"$nulls":11},263,"est time"]
[]
[]
["valery m","cs-ring",37,"2004-06-30",null,null,"fast luminosity monitor q3w quad sup"]
[{"$nulls":6},"cross plate-1","6041-159-0101","steel",1,6,6,"mill",null,"rs","2004-07-22","hold"]
[{"$nulls":6},"cross plate-2","6041-159-0102","steel",1,6,6,"mill",null,"rs","2004-07-22","hold"]
[{"$nulls":6},"main plate","6041-159-0103","steel",1,8,8,"mill",null,"ds","2004-07-15","done"]
[{"$nulls":6},"push-pull block","6041-159-0104","ss",3,3,9,"mill",null,"tr","2004-07-07","done"]
[{"$nulls":6},"screw modification","6041-159-0105","steel",3,0.5,1.5,"lathe",null,"rm","2004-07-29","done"]
[{"$nulls":6},"pad-1","6041-159-0201","steel",1,16,16,"mill",null,"ds","2004-07-15","done"]
[{"$nulls":6},"pad-2","6041-159-0202","steel",1,16,16,"mill",null,"ds","2004-07-15","done"]
[{"$nulls":6},"clamp bar-1","6041-159-0203","ss",2,3,6,"mill",null,"austin","2004-07-27","done"]
[{"$nulls":6},"clamp bar-2","6041-159-0204","ss",2,3,6,"mill",null,"austin","2004-07-27","done"]
[{"$nulls":6},"clamp bar-3","6041-159-0205","ss",1,3,3,"mill",null,"austin","2004-07-27","done"]
[{"$nulls":6},"clamp bar-4","6041-159-0206","ss",1,3,3,"mill",null,"austin","2004-07-27","done"]
[{"$nulls":6},"cross bar","6041-159-0207","ss",1,2,2,"mill",null,"austin","2004-07-27"]
[{"$nulls":6},"main clamp bar","6041-159-03","ss",2,3,3,"mill",null,"austin","2004-07-27"]
[{"$nulls":11},85.5,"est time"]
[]
["vadim v","hc",39,"2004-07-29",null,null,"erl injector coupler","2 assy"]
[{"$nulls":6},"antenna tube","7102-003-0102","cu",2,3,6,"lathe"]
[{"$nulls":6},"screw","7102-003-0103","cu",2,4,8,"lathe"]
[{"$nulls":6},"central tube","7102-003-0201","cu",2,5,10,"lathe"]
[{"$nulls":6},"screw","7102-003-0202","ss",2,4,8,"lathe"]
[{"$nulls":6},"nut","7102-003-0203","ss",2,3,6,"lathe"]
[{"$nulls":6},"flange","7102-003-0601","ss",2,6,12,"lathe"]
[{"$nulls":6},"taper","7102-003-0602","cu",2,8,16,"lathe"]
[{"$nulls":6},"tube","7102-003-0603","cu",2,3,6,"lathe"]
[{"$nulls":6},"7/8\" eia flange","7102-003-0604","ss",2,4,8,"lathe"]
[{"$nulls":6},"teflon insulator 1","7102-003-04","teflon",2,3,6,"lathe"]
[{"$nulls":6},"inner rod","7102-003-05","cu",2,7,14,"lathe"]
[{"$nulls":11},100,"est time"]
[]
["jim s","s-ring",40,"2004-07-29",null,null,"mk3 cryostat","1 assy"]
[{"$nulls":5},22,"fbt thermx left flange","5055-056-22","ss",1,24,24,"lathe/cnc-mill"]
[{"$nulls":5},23,"fbt thermx right flange","5055-056-23","ss",1,20,20,"lathe/cnc-mill"]
[{"$nulls":5},24,"fluted segment","5055-056-24","ss",4,10,40,"press"]
[{"$nulls":5},"   25-1","liquid n2 flange","5055-056-25","cu",1,10,10,"lathe/cnc-mill"]
[{"$nulls":5},"   25-2","rf probe housing","5055-056-25","ss",4,2,8,"lathe/cnc-mill"]
[{"$nulls":6},"make dies for pressing fluted seg",null,null,"   1+1",10,20,"cnc-mill"]
[{"$nulls":11},122,"est time"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}